{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":6,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":192,"n_cols":13,"rows_kept":192,"cut":false,"hidden":false,"merged":[[2,0,2,5]],"flags":["formulas_cached_only"]}
["Revised: December 10th, 2014"]
["Revision: Production, EAH Jena Lötlabor"]
["Bill Of Materials       "]
["Item","Qty","Part Number","Value","Ref.Des.","PCB Footprint","Manufacturer","Vendor","Vendor PN","Qty","ordered","checked","comment"]
[]
[1,4,"08055A100JAT2A","10pF","C1,C2,C28,C29",805,"AVX","DigiKey","478-1304-1-ND",4,4,"ok"]
[2,31,"T491A106M020AT","10uF","C3,C5,C8,C9,C16,C17,C18,","3216-18 (EIA)","Kemet","Reichelt","X7R-G1206 10/25",31,35,"ok","see Item 19"]
[{"$nulls":4},"C20,C21,C30,C31,C51,C56,"]
[{"$nulls":4},"C58,C77,C78,C125,C152,"]
[{"$nulls":4},"C164,C168,C171,C172,C175,"]
[{"$nulls":4},"C188,C203,C219,C220,C221,"]
[{"$nulls":4},"C223,C224,C226"]
[3,106,"C0805X104K1RACTU","100nF","C4,C7,C11,C14,C15,C19,",805,"Kemet","Reichelt","X7R-G0805 100N",106,107,"ok"]
[{"$nulls":4},"C23,C24,C25,C26,C27,C33,"]
[{"$nulls":4},"C35,C36,C38,C41,C43"]
[{"$nulls":4},"C44,C45,C46,C47,C48,C50,"]
[{"$nulls":4},"C52,C54,C55,C61,C63,C64,"]
[{"$nulls":4},"C65,C66,C67,C68,C69,C71,"]
[{"$nulls":4},"C74,C76,C79,C81,C83,C84,"]
[{"$nulls":4},"C86,C89,C90,C92,C93,C94,"]
[{"$nulls":4},"C96,C97,C98,C99,C101,"]
[{"$nulls":4},"C104,C106,C111,C115,C116,"]
[{"$nulls":4},"C117,C118,C119,C120,C122,"]
[{"$nulls":4},"C123,C124,C134,C135,C137,"]
[{"$nulls":4},"C138,C139,C142,C145,C148,"]
[{"$nulls":4},"C153,C154,C155,C156,C158,C161,C163,"]
[{"$nulls":4},"C165,C166,C169,C170,C173,"]
[{"$nulls":4},"C176,C182,C183,C189,C190,"]
[{"$nulls":4},"C192,C193,C197,C199,C200,"]
[{"$nulls":4},"C202,C204,C206,C208,C210,"]
[{"$nulls":4},"C211,C212,C214,C215,C216,"]
[{"$nulls":4},"C218,C227"]
[4,40,"GRM21BR72A103KA01L","10nF","C6,C10,C42,C53,C59,C82,",805,"Murata","DigiKey","490-1652-1-ND",40,50,"ok"]
[{"$nulls":4},"C85,C91,C95,C102,C108,"]
[{"$nulls":4},"C109,C110,C112,C113,C114,"]
[{"$nulls":4},"C121,C126,C127,C128,C129,"]
[{"$nulls":4},"C130,C131,C136,C140,C141,"]
[{"$nulls":4},"C143,C144,C146,C147,C151,C157"]
[{"$nulls":4},"C159,C160,C162,C167,C201,R145,R102"]
[{"$nulls":4},"C217"]
[5,1,"GRM2165C2A201JA01D","200pF","C12",805,"Murata","DigiKey","490-1606-1-ND",1,1,"ok"]
[6,1,"SG2020CT-ND","20pF","C13","TRIMMER","Sprague","Reichelt","TZC03 20P",1,1,"ok"]
[7,1,"08055A150JAT2A","15pF","C22",805,"AVX","DigiKey","478-1306-1-ND",1,1,"ok"]
[8,1,"C0805X104K1RACTU","100nF ","C39",805,"Kemet","Reichelt",null,1,null,"ok","see Item 3"]
[9,15,"C2012C0G1H102J","1nF","C40,C49,C60,C62,C72",805,"TDK","DigiKey","445-1330-1-ND",15,15,"ok"]
[{"$nulls":4},"C73,C80,C100,C103,C107,"]
[{"$nulls":4},"C132,C133,C179,C180"]
[10,2,"08055A330JAT2A","33pf","(C37,C39)",805,"AVX","Reichelt","NPO-G0805 33P",2,2,"ok"]
[11,3,"B45197A5476K409","47uF","C57,C177,C198","7343-31 (EIA)","Kemet","Reichelt","X5R-G1206 47/6",3,3,"ok"]
[12,3,"C0805C101J5GACTU","100pF","C75,C87,C105",805,"Kemet","DigiKey","399-1122-1-ND",3,3,"ok"]
[13,1,"TMK212B7225KG-TR","2.2uF","C88",805,"Taiyo Yuden","DigiKey","587-2991-1-ND",1,1,"ok"]
[14,1,"GRM21BR71E334KA01L","330nF","C149",805,"Murata","DigiKey","490-1677-1-ND",1,1,"ok"]
[15,1,"08055C473KAT2A","47nF","C150",805,"AVX","DigiKey","478-1391-1-ND",1,1,"ok"]
[16,7,"TAJA105K025RNJ","1uF","C174,C205,C207","3216-18 (EIA)","AVX","Reichelt","X7R-G1206 1,0/50",7,7,"ok"]
[{"$nulls":4},"C209,C213,C222,C225"]
[17,2,"C2012Y5V1H105Z","1uf","C178,C181",805,"TDk","DigiKey","445-1354-1-ND ",2,2,"ok"]
[18,1,"08055C473KAT2A",".47uf","C185",805,"TDK","DigiKey","445-1353-1-ND",1,1,"ok"]
[19,4,"EMK212BJ106KG-T","10uf","C184,186,194,195",805,"TDk","Reichelt","X7R-G1206 10/25",4,4,"ok","see Item 2"]
[20,1,"GRM2165C1H471JA01D","470pF","C191",805,"Murata","DigiKey","490-1617-1-ND",1,1,"ok"]
[21,1,"GRM2165C1H681JA01D","680pf","C187",805,"MURATA","DigiKey","490-1619-1-ND",1,1,"ok"]
[22,1,"GRM216F51E474ZA01D","470nF","C196",805,"Murata","DigiKey","490-3346-1-ND",1,1,"ok","see Item 18"]
[23,2,"LS Y876-Q2S1-1-Z","RED_RA","D1,D6",1210,"Osram","DigiKey","475-2769-1-ND",2,2,"ok"]
[24,2,"BAT54C-G","BAT54C","D7,D2","SOT23A","Comchip","DigiKey","641-1320-1-ND",2,2,"ok"]
[25,1,"BAT54S-TP","BAT54S","D3","SOT23A","Micro Commercial","DigiKey","BAT54STPMSCT-ND",1,1,"ok"]
[26,3,"BAT54-TP","BAT54","D4,D5,D24","SOT23A","Micro Commercial","DigiKey","BAT54TPMSCT-ND",3,3,"ok"]
[27,1,"BAT54A-G","BAT54A","D8","SOT23A","Comchip","DigiKey","641-1319-1-ND",1,1,"ok"]
[28,1,"652-CDSOD323-T05LC","652-CDSOD323-T05LC","D9","SOD323","Bourns",null,"BAV99?",1,null,"not ok"]
[29,15,"APT2012SURCK","RED","D10,D11,D12,D13,D14,D15,","LED (0805)","Kingbright","DigiKey","754-1133-1-ND",15,15,"ok"]
[{"$nulls":4},"D16,D17,D18,D19,D23,D25,"]
[{"$nulls":4},"D26,D27,D28"]
[30,3,"MBRA340T3G","MBRA340","D20,D22,D29","DO-214AC","ON Semi",null,"!!TODO!!",3,null,"not ok","SMPS diodes"]
[31,1,"BZX84C3V3-TP","BZX84C3V3","D21","SOT23A","Micro Commercial","DigiKey","BZX84C3V3-TP-ND",1,1,"ok"]
[null,8,"none","FIDUCIAL DNI","FD1,FD2,FD3,FD4,FD5,FD6,","FIDUCIAL","none","none","none",8,null,"ok"]
[{"$nulls":4},"FD7,FD8"]
[32,1,"RLP-50+","RLP-40+","FL1","PL-176 (fl1)","Mini-Circuits","Mini-Circuits","RLP-40+",1,0,"not ok","MC"]
[33,17,"EXC-CET102U","EXC-CET102U","FL2,FL3,FL4,FL5,FL7,FL8,","INDUCTOR AUDIO (P9830TR-ND)","Panasonic","DigiKey",null,17,0,"ok","use FB"]
[{"$nulls":4},"FL9,FL10,FL11,FL12,FL13,"]
[{"$nulls":4},"FL14,FL15,FL16,FL17,FL18,"]
[{"$nulls":4},"FL19"]
[34,1,"LFCV-52+","LFCV-52+","FL20","LFCV-52+","MINI CIRCUITS","Mini-Circuits","LFCV-52+",1,0,"not ok","MC"]
[35,1,"RLP-50+","RLP-50+","FL6","PL-176 (fl1)","Mini-Circuits","Mini-Circuits","RLP-50+",1,0,"not ok","MC"]
[36,3,null,"2A","F1,F2,F3",1812,"Bel Fuse",null,"1A SMD Fuse",3,null,"ok","existing"]
["36A",2,"22-28-4020","JMP_2P - DNI","JP1,JP2","2 PIN BERG","Molex","Reichelt","SL 1X50G 2,54","x",1,"ok"]
[37,5,"22-28-4030","JMP_3P","JP4,JP5,JP6,J17,J26","3 PIN BERG","Molex","Reichelt",null,"x","x","ok","see Item 36A"]
[38,1,"142-0701-501","SMA_F_RA ","J1","SMA (SMA_Right angle)","Emerson","Reichelt",null,1,0,"ok","not pop."]
[39,3,"SJ1-3533","3.5MM STEREO RA","J2,J4,J6","3.5MM STEREO AUDIO JACK (Right angle_drill1.9)","CUI","DigiKey","CP1-3533-ND",3,0,"ok","not pop."]
[40,3,"142-0701-501","SMA_F_RA","J3,J5,J25","SMA (SMA_Right angle)","Emerson","Reichelt","SMA BU P",3,3,"ok"]
[41,2,"10-89-7101","HDR 10P DUAL","P2,P1","10 PIN BERG","Molex","Reichelt","SL 2X50G 2,54","x",1,"ok"]
[42,2,"22-27-2031","HDR 3P SGL VERT","J9,J8","SPEAKER","Molex","DigiKey","WM4112-ND",2,2,"ok"]
[43,1,"640454-4","4 Pin","J10","DC CONNECTOR (12V IN_a_pankaj)","TE","DigiKey","A19431-ND",1,1,"ok"]
[44,8,"22-28-4020","JMP_2P","J11,J12,J13,J18,J21,J22,","2 PIN BERG","Molex","Reichelt",null,"x","x","ok","see Item 36A"]
[{"$nulls":4},"J23,J24"]
[45,1,"22-28-4050","HDR 5P SGL","J14","5 PIN BERG","Molex","Reichelt",null,"x","x","ok","see Item 36A"]
[46,1,"10-89-7101","HDR 10P DUAL - ","J15(ALEX HDR 10P)","10 PIN BERG","Molex","Reichelt",null,"x","x","ok","see Item 41"]
[47,1,"10-89-7302","HDR 26P DUAL VERT - ","J16","26 PIN BERG (2x15)","Molex","Reichelt","WSL 26W",1,1,"ok"]
[48,1,"22-28-4040","HDR 4P SGL","J19","4 PIN BERG","Molex","Reichelt",null,"x","x","ok","see Item 36A"]
[49,1,"10-89-7041","JMP_4P","J20","2X2 BERG","Molex","Reichelt",null,"x","x","ok","see Item 36A"]
[50,2,"128-0711-201","UMC","J28,J29","UMC","Emerson","DigiKey","J983-ND",2,0,"ok","not pop."]
[51,1,"SJ1-3533NG","3.5MM STEREO RA INSUL ","J27","3.5MM STEREO AUDIO JACK (Right angle_drill1.9)","CUI","DigiKey","CP1-3533NG-ND",1,0,"ok","not pop."]
[52,20,"445-1568-2-ND","220 OHM (FERRITE CHIP)","L1,L2,L6,L8,L9,L10,L11",805,"TDK","DigiKey","445-1568-1-ND",20,20,"ok"]
[{"$nulls":4},"L12,L14,L15,L16,L18,L19,L20"]
[{"$nulls":4},"L21,L22,L23,L30,L31,L33"]
[53,1,"ELJ-NDR56JF","560nH","L3",805,"Panasonic","DigiKey","PCD1181CT-ND",1,1,"ok"]
[54,1,"AISC-0805-R022J-T","22nH","L4",805,"Abracon","DigiKey","535-10493-1-ND",1,1,"ok"]
[55,2,"AISC-0805-R047J-T","47nH","L17,L13",805,"Abracon","DigiKey","535-10497-1-ND",2,2,"ok"]
[56,4,2743021447,"FB_2743021447","L24,L25,L27,L32","Inductor","Fair-Rite",null,"FB",4,null,"ok","use FB"]
[57,2,"NFM41PC204F1H3L","200nF","L26,L29","RFC (UPDATED1)","Murata","DigiKey","490-2550-1-ND",2,2,"ok"]
[58,1,"VLC6045T-4R7M","4.7uH","L28",null,"TDK","DigiKey","445-6538-1-ND",1,1,"ok"]
[]
[59,1,"6605444-6","RJ45","J7","RJ45-PHY","TE Connectivity",null,"!!TODO!!",1,null,"not ok","RJ45"]
[60,2,"2N7002K","2N7002K","Q1,Q2","SOT23A","Fairchild","DigiKey","2N7002KCT-ND",2,2,"ok"]
[61,2,"MMBT3906-7-F","MMBT3906-7-F","Q3,Q4","SOT23A","NXP","DigiKey","MMBT3906-TPCT-ND",2,2,"ok"]
[62,6,"CRCW08051K50FKEA","1K5","R1,R19,R115,R116,R117,",805,"Vishay",null,"1k5",6,null,"ok","existing"]
[{"$nulls":4},"R118"]
[63,1,"ERJ-6GEYJ153V","15k","R111",805,"PANASONIC","DIGIKEY","P15KACT-ND",1,1,"ok"]
[64,28,"CRCW080510K0FKEA","10K","R2,R10,R40,R41,R42,R50,",805,"Vishay",null,"10k",28,null,"ok","existing"]
[{"$nulls":4},"R52,R53,R54,R58,R64,R65,"]
[{"$nulls":4},"R66,R67,R68,R69,R70,R71,"]
[{"$nulls":4},"R72,R74,R75,R78,R80,R81,"]
[{"$nulls":4},"R82,R106,R108,"]
[{"$nulls":4},"R122"]
[65,15,"CRCW08051K00FKEA","1K","R3,R16,R21,R26,R43,R48,",805,"Yageo","DigiKey","311-51ARCT-ND",15,15,"ok"]
[{"$nulls":4},"R49,R61,R79,R85,R103"]
[{"$nulls":4},"R109,R114,R120,R121,R130"]
[66,6,"CRCW080522R0FKEA","22E","R4,R25,R28,R29,R33,R34",805,"Vishay","DigiKey","541-22.0CCT-ND",6,10,"ok","too much"]
[67,12,null,"2K2","R5,R6,R88,R89,R90,R91,",805,"Panasonic","DigiKey","P2.20KCCT-ND",12,12,"ok"]
[{"$nulls":4},"R92,R93,R94,R95,R96,R97"]
[68,2,"CRCW080551R0FKEA","51E","R143,R7",805,"Vishay","DigiKey","541-51.0CCT-ND",2,10,"ok","see Item 82"]
[69,1,"CRCW08051K80FKEA","1K8","R8",805,"Vishay","DigiKey","541-1.80KCCT-ND",1,10,"ok","too much"]
[70,1,"CRCW080518K0FKEA","18K","R9",805,"Vishay","DigiKey","541-18.0KCCT-ND",1,10,"ok","too much"]
[71,2,"CRCW0805510KFKEA","510K","R12,R11",805,"Vishay","DigiKey","541-510KCCT-ND",2,10,"ok","too much"]
[72,4,"CRCW0805100KFKEA","100K","R13,R14,R15,R112",805,"Vishay",null,"100R",4,null,"ok","existing"]
[null,null,"DNI","DNI","R18,R17",805,"Vishay",null,"DNI",null,null,"ok"]
[73,5,"CRCW08053K30FKEA","3K3","R20,R76,R129,R138,R140",805,"Vishay","DigiKey","541-3.30KCCT-ND",5,10,"ok","too much"]
[74,3,"CRCW0805100RFKEA","100E","R22,R24,R141",805,"Vishay","DigiKey","541-100CCT-ND",3,10,"ok","too much"]
[75,1,"CRCW0805220KFKEA","220K","R23",805,"Vishay","DigiKey","541-220KCCT-ND",1,10,"ok","too much"]
[76,1,"CRCW0805200RFKEA","200E","R27",805,"Vishay","DigiKey","541-200CCT-ND",1,10,"ok","too much"]
[77,2,"CRCW0805330RFKEA","330E","R30,R31",805,"Vishay","DigiKey","541-330CCT-ND",2,10,"ok","too much"]
[78,1,"CRCW0805220RFKEA","220E","R32",805,"Vishay","DigiKey","541-220CCT-ND",1,10,"ok","too much"]
[79,3,"CRCW0805470RFKEA","470 OHM","R35,R36,R37",805,"Vishay",null,"470R",3,null,"ok","existing"]
[80,2,"CRCW0805270RFKEA","270E","R142",805,"Vishay","DigiKey","541-270CCT-ND",2,10,"ok","too much"]
[81,2,"CRCW08054R70FKEA","4.7E","R39,R38",805,"Vishay","Reichelt","SMD-0805 4,70",2,2,"ok"]
[82,2,"CRCW080551R0FKEA","51 OHM","R44,R45",805,"Vishay","DigiKey","541-51.0CCT-ND",2,null,"ok","see Item 68"]
[83,1,"CRCW08051M00FKEA","1M","R46",805,"Vishay",null,"1M",1,null,"ok","existing"]
[84,9,"CRCW08050000Z0EA"," RES 0 OHM","R47,R51,R60,R62,R63,R84",805,"Vishay",null,"0R",9,null,"ok","existing"]
[{"$nulls":4},"R86,R119,R123"]
[85,3,"CRCW0805220RFKEA","220E","R55,R56,R127",805,"Vishay","DigiKey","541-220CCT-ND",3,null,"ok","see Item 78"]
[86,1,"CRCW08054K99FKEA","4K99","R57",805,"Vishay","DigiKey","541-4.99KCCT-ND",1,10,"ok","too much"]
[87,3,"CRCW08054K70FKEA","4K7","R59,R73,R104",805,"Vishay",null,"4k7",3,null,"ok","existing"]
[88,8,"CRCW08050000Z0EA","RES 0 OHM","R77,R87,R131,R132,R133,",805,"Vishay",null,"0R",8,null,"ok","existing"]
[{"$nulls":4},"R135,R136,R137"]
[89,1,"CRCW080547K0FKEA","47K","R83,R101,R107",805,"Vishay",null,"47k",1,null,"ok","existing"]
[90,4,"CRCW080533R0FKEA","33E","R98,R99,R100,R105",805,"Vishay",null,"33R",4,null,"ok","existing"]
[91,1,"CRCW0805820RFKEA","820 OHM","R110",805,"Vishay","DigiKey","541-820CCT-ND",1,10,"ok","too much"]
[92,1,"CRCW080512K0FKEA","63.4K","R113",805,"Vishay","DigiKey","P63.4KCCT-ND",1,10,"ok","too much"]
[93,1,"CRCW080510K0FKEA"," RES 10K ","R124",805,"Vishay",null,"10k",1,null,"ok","existing"]
[94,1,"CRCW0805270KFKEA","536k","R125",805,"Vishay","DigiKey","541-536KCCT-ND",1,10,"ok","too much"]
[95,2,"CRCW08056K80FKEA","6K8","R128,R139",805,"Vishay",null,"6k8",2,null,"ok","existing"]
[96,2,"CRCW0805120RFKEA","120  OHM","R134,R144",805,"Vishay","DigiKey","541-120CCT-ND",2,10,"ok","too much"]
[null,5,"none","PLT HOLE  DNP","SC1,SC2,SC3,SC4,SC5","MHOLEP5D4","none","none","none",5]
[97,1,"P227EE1CXC","DPST OFF-ON - ","SW1","POWER SWITCH EG1026-ND","E-Switch","DigiKey","EG1026-ND",1,1,"ok"]
[98,2,"TC1-1TG2+","TC1-1TG2+","T5,T1","AT224","Mini-Circuits","Mini-Circuits","TC1-1TG2+",2,null,"not ok","MC"]
[99,2,"TC4-1T+","TC4-1T+","T4,T2","AT224","Mini-Circuits","Mini-Circuits","TC4-1T+",2,null,"not ok","MC"]
[100,1,"ADT1.5-1+","ADT1.5-1+","T3","CD542","Mini-Circuits","Mini-Circuits","ADT1.5-1+",1,null,"not ok","MC"]
[101,1,"M25P16-VMW6G","M25P16VMW6G","U1","SOIC-8","Numonyx","DigiKey","M25P16-VMN6TPCT-ND",1,1,"ok"]
[102,1,"TLV320AIC23BIPWR","TLV320AIC23B","U2","TSSOP-28","TI","DL3YC","TLV320AIC23B",1,null,"ok","existing"]
[103,2,"LMC6482AIM/NOPB","LM6482AM","U3,U4","SOIC-8","NSC","DigiKey","LMC6482AIM-ND",2,2,"ok"]
[104,1,"AD9744ARUZ","AD9744ARU","U5","TSSOP-28","Analog Devices","DigiKey","AD9744ARUZ-ND",1,1,"ok"]
[105,2,"OPA2674ID","OPA2674ID","U7,U6","SOIC-8","TI","DigiKey","296-15212-5-ND",2,2,"ok"]
[106,1,"FOX924B-25.000","TCXO 25MHz","U8","SMD 5mm x 3.2mm5MM","Fox","DigiKey","631-1074-1-ND",1,1,"ok"]
[107,1,"EP3C40Q240C8N","EP3C40Q240","U9","PQFP-240","Altera","DigiKey","544-2551-ND",1,1,"ok"]
[108,1,"LTC2208CUP#PBF","LTC2208CUP","U10","QFN-64 (UPDATED2)","Linear Tech","DigiKey","LTC2208CUP#PBF-ND",1,1,"ok"]
[109,1,"LTC6400CUD-20#PBF","LTC6400-20","U11","QDN-16","Linear Tech","DigiKey","LTC6400CUD-20#PBF-ND",1,1,"ok"]
[110,1,"DAT-31-SP+","DAT-31-SP+","U12","QFN-20","Mini-Circuits","Mini-Circuits","DAT-31-SP+",1,null,"not ok","MC"]
[111,1,"KSZ9021RL","KSZ9021RL","U13","LQFP-64","Micrel","DigiKey","576-3439-ND",1,1,"ok"]
[112,1,"SN65LVDM180D","SN65LVDM180D","U14","SOIC-14","TI","DigiKey","296-1420-5-ND",1,1,"ok"]
[113,1,"25AA02E48T-I/OT","25AA02E48","U15","SOT-23-6","Microchip","DigiKey","25AA02E48T-I/OTCT-ND",1,1,"ok"]
[114,1,"CVHD-950-122.880","TCXO 122.88MHz","U16","SMD 14mm x 9mm","Crystek","DigiKey","744-1271-ND",1,1,"ok"]
[115,1,"ADC78H90CIMT/NOPB","ADC78H90CIMT","U17","16-TSSOP","National","DigiKey","ADC78H90CIMT/NOPB-ND",1,1,"ok"]
[116,1,"NCP1117ST12T3G","NCP1117ST12T3G","U18","SOT-223","ON Semi","DigiKey","NCP1117STAT3GOSCT-ND",1,1,"ok","adj version!"]
[117,2,"LD1117AS12TR","LD1117-1.2V","U30,U19","SOT-223","ST Micro","DigiKey","497-6445-1-ND",2,2,"ok"]
[118,2,"74LCX541MTC","74LCX541","U25,U20","TSSOP-20","Fairchild","DigiKey","74LCX541MTC-ND",2,2,"ok"]
[119,1,"TPA0202PWP","TPA0202PWP","U21","TPA0202 (TSSOP-24centrepth )","TI","DigiKey","296-1940-5-ND",1,1,"ok"]
[120,1,"ULN2003AD","ULN2003AD","U22","SOIC-16","TI","DigiKey","296-1368-5-ND",1,1,"ok"]
[121,1,"LT1529CQ-3.3#PBF","LT1529-3.3V","U23","Q PACKAGE (UPDATE2)","Linear Tech","DigiKey","LT1529CQ-3.3#PBF-ND",1,1,"ok"]
[122,1,"LT3680EDD#PBF","LT3680","U24","DFN (UPDATED)","Linear Tech","DigiKey","LT3680EMSE#PBF-ND",1,1,"ok"]
[123,1,"FOX924B-10.000","TCXO 10MHz","U26","SMD 5mm x 3.2mm5MM","Fox","DigiKey","631-1067-1-ND",1,1,"ok"]
[124,1,"LD1117S25TR","LD1117-2.5V","U27","SOT-223","ST Micro","DigiKey","497-7309-1-ND",1,1,"ok"]
[125,4,"LD1117S33CTR","LD1117-3.3V","U28,U29,U31,U32","SOT-223","ST Micro","DigiKey","497-1241-1-ND",4,4,"ok"]
[126,null,"Case",{"$nulls":4},"DigiKey","HM1114-ND",1,1,"ok"]
[]
[{"$nulls":5},"Note 1 - R102, R145 are 0E bypass resistors in case you do not want to use SW1, if \nusing SW1 they can either\nbe populated by 10nf caps or left unpopulated"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}